ACMS API Guide

Release 0.1

**VERSION’S HISTORY**

| **Version** | **Date** | **Creator** | **Modifications object** |
| --- | --- | --- | --- |
|  |  |  |  |

M-must 必须填写的域 O-option 自选填写的域 C-conditional 某条件成立时必须填写的域

## Get Charging status

### Purpose

Get charging status .

### Access:

**HTTP Verb :** GET

**Request URL :** <https://acmstest.nissan.com.cn/smallev/carmodel>？carModelID=${CarModelID}

### Input format

|  |  |  |  |
| --- | --- | --- | --- |
| **Attributes** | **M/O/C** | **Format** | **Description / Comments** |
| carModelID | M | String | - |

### Input sample

### Output format

|  |  |  |  |
| --- | --- | --- | --- |
| **Attributes** | **M/O/C** | **Format** | **Description / Comments** |
| status | M | int | 0:not charging 1:int the charging 2:charge complete 3: exception |
| soc | m | int | 0~100 |

### Output sample

Success sample

{

"status": 0

}